[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A14. CHECK FLUID LEVEL IN BRAKE RESERVOIR | PRINT PAGE / INDEX / PRIOR / NEXT

| A14. CHECK FLUID LEVEL IN BRAKE RESERVOIR
| Check that the fluid level is between the "MAX" and "MIN" or "A" mark. If it is below the "MIN" or "A" marks, replenish with fresh brake fluid up to the "MAX" mark.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A14. CHECK FLUID LEVEL IN BRAKE RESERVOIR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation