[23A] AUTOMATIC TRANSMISSION (FF) - - TRANSMISSION CONTROL <R.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

TRANSMISSION CONTROL <R.H. DRIVE VEHICLES>

REMOVAL AND INSTALLATION
WARNING When removing and installing the transmission control cable and shift lock cable unit, be careful not to hit the SRS-ECU.
Pre-removal and Post-installation Operation Instrument Panel Centre Console Removal and Installation (Refer to GROUP 52A - Instrument Panel assembly .)
|  |  | Selector lever assembly and transmission control cable assembly removal steps
--- | --- | --- | ---
|  | • | Footrest
| >>B<< | 1. | Transmission control cable connection (Transmission side)
| >>A<< | 2. | Shift lock cable unit connection <For South Africa, Hong Kong, Brunei, Singapore, Malaysia and New Zealand (4G63 engine)>
|  | 3. | Transmission control cable connection (shift lever side)
|  | 4. | Shift switch connector
|  | 5. | Selector lever assembly
|  | • | Air cleaner (Refer to GROUP 15 - Air cleaner <4G63-SOHC, 4G64>, GROUP 15 - Air cleaner <4G63-DOHC>, .GROUP 15 - Air cleaner <4G69>.)
|  | • | Battery and Battery tray
|  | • | SRS-ECU (Refer to GROUP 52B - SRS air bag control unit .)
|  | 6. | Transmission control cable assembly (Selector lever side)
| INSTALLATION SERVICE POINTS
| >>A<< SHIFT LOCK CABLE UNIT INSTALLATION <FOR SOUTH AFRICA, HONG KONG, BRUNEI, SINGAPORE, MALAYSIA AND NEW ZEALAND (4G63 ENGINE) > Shift the selector lever to the P position and turn the ignition switch to the LOCK (OFF) position.
| After installing the rod of the shift lock cable unit to the lock cam of the selector lever assembly, tighten the bolts of the shift lock cable unit to the specified torque. Tightening torque: 5.0 ± 1.0 N·m Check the operation of the selector lever. (Refer to .)
| >>B<< TRANSMISSION CONTROL CABLE (TRANSMISSION SIDE) INSTALLATION Shift the selector lever and manual control lever to the N position.
| Gently push the transmission control cable in the direction of the arrow to tighten the adjusting nut to the specified torque. Tightening torque: 12 ± 2 N·m

[23A] AUTOMATIC TRANSMISSION (FF) - - TRANSMISSION CONTROL <R.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation