[54A] CHASSIS ELECTRICAL - - BATTERY - ON-VEHICLE SERVICE - BATTERY TEST | PRINT PAGE / INDEX / PRIOR / NEXT

BATTERY TEST
BATTERY TESTING PROCEDURE
STEP 1. Check the battery cables. Remove the negative cable, then the positive cable. Check for dirty or corroded connections. Q: Are the battery cables dirty or have corroded connections? YES: Clean the battery cables. Then go to Step 2. NO: Go to Step 2.
STEP 2. Check the battery post. Check for loose battery post. Q: Are the battery post faulty? YES: Replace the battery. Then go to Step 4. NO: Go to Step 3.
STEP 3. Check the battery case and cover. Remove the hold-downs and shields. Check for broken/cracked case or cover. Q: Is the battery case or cover faulty? YES: Replace the battery. Then go to Step 4. NO: Go to Step 4.
STEP 4. Check the open circuit voltage. Turn headlamps on for 15 seconds. Turn headlamps off for two minutes to allow battery positive voltage to stabilize. Disconnect the battery cables. Read open circuit voltage. Q: Is open circuit voltage 12.4 volts or more? YES: Go to Step 5. NO: Charge the battery at 5 amps for 15 hours. Then re-test.
STEP 5. Check the load test. Connect a load tester to the battery. Load the battery at the recommended discharge rate (See LOAD TEST RATE CHART) for 15 seconds. Read voltage after 15 seconds, then remove load. Compare the measured value with the minimum voltage (See LOAD TEST CHART). Q: Is the voltage higher than minimum voltage? YES: The battery is normal. NO: Replace the battery. Then go to Step 4.
LOAD TEST CHART
Temperature °C | 21 and above | 16 | 10 | 4 | -1 | -7 | -12 | -18
--- | --- | --- | --- | --- | --- | --- | --- | ---
Minimum voltage | 9.6 | 9.5 | 9.4 | 9.3 | 9.1 | 8.9 | 8.7 | 8.5
LOAD TEST RATE CHART
Battery type | 44B20L <Vehicles for Hong Kong, Brunei, Singapore, Malaysia> | 75D23L <Vehicles for General Export (except for Hong Kong, Brunei, Singapore, Malaysia), GCC, Australia and New zealand (2400)> <Option for Hong Kong, Brunei, Singapore, Malaysia>
--- | --- | ---
Charging time when fully discharged h (5-anp. rated current charging) | 7 | 11
Load test (Amps) | 215 | 275

[54A] CHASSIS ELECTRICAL - - BATTERY - ON-VEHICLE SERVICE - BATTERY TEST | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation