[51] EXTERIOR - - OUTSIDE MIRROR - DOOR MIRROR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

DOOR MIRROR

REMOVAL AND INSTALLATION
|  |  | Door mirror removal steps
--- | --- | --- | ---
|  | 1. | Delta cover
|  | 2. | Tweeter
| >>A<< | 3. | Door mirror assembly
|  | 4. | Door mirror body assembly
<<A>> |  | 5. | Mirror
|  |  | Remote controlled mirror switch removal steps
|  | 6. | Instrument panel lower cover (Refer to GROUP 52A, Instrument panel <L.H. drive vehicles>, <R.H. drive vehicles>).
|  | 7. | Remote controlled mirror switch
| REMOVAL SERVICE POINT
| <<A>> MIRROR REMOVAL
| CAUTION The claw of the mirror is prone to breakage when working in cold temperatures. Always warm up the mirror claw and claw periphery to 20°C or higher before handling. Slant the mirror upward with your hands. Then insert a flat-tipped screwdriver wrapped with protective tape between the pivot plate and mirror through the cut-out from behind the mirror. Now pry off the mirror claw and remove the mirror as shown.
| INSTALLATION SERVICE POINT
| >>A<< DELTA COVER INSTALLATION
| CAUTION If the delta cover is placed with the clip on the door panel, the clip may be pushed into the door panel and fall off. Thus, special care is necessary. Install the delta cover with the clip installed.
| >>B<< DOOR MIRROR ASSEMBLY INSTALLATION
| CAUTION When assembling the door mirror, check to see that the claw of the door mirror is inserted in the notch of the front door runchannel.

[51] EXTERIOR - - OUTSIDE MIRROR - DOOR MIRROR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation