[54A] CHASSIS ELECTRICAL - - REAR COMBINATION LAMP - REAR COMBINATION LAMP DIAGNOSIS | PRINT PAGE / INDEX / PRIOR / NEXT

REAR COMBINATION LAMP DIAGNOSIS
The lamps setup on the rear combination lamp is controlled in the same manner as the lamps of the headlamp assembly. For details go to the reference. For troubleshooting, refer to respective Groups below. Not using SWS monitor <Hong Kong spec.>: GROUP 54B, Troubleshooting . Using SWS monitor <Hong Kong spec.>: GROUP 54C, Troubleshooting . Not using SWS monitor <Except for Hong Kong spec.>: GROUP 54D, Troubleshooting . Using SWS monitor <Except for Hong Kong spec.>: GROUP 54E, Troubleshooting .

[54A] CHASSIS ELECTRICAL - - REAR COMBINATION LAMP - REAR COMBINATION LAMP DIAGNOSIS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation