[55] HEATER, AIR CONDITIONER AND VENTILATION - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
The heater and air conditioner system incorporating the heater and cooling unit has reduced ventilation resistance to increase air volume and reduce noise. The manual air conditioner has been adopted. <except for Hong Kong, Brunei, Singapore, Malaysia and South Africa> The automatic air conditioner has been adopted to the vehicles for Hong Kong, Brunei, Singapore, Malaysia, South Africa and New Zealand.
FEATURES
IMPROVEMENTS IN COMFORT Installation of two-layer blow full air mix heater Adoption of low noise, large air volume heater and air conditioner system
IMPROVEMENTS IN OPERATION PERFORMANCE Large rotary control to improve controllability Enlarging the figures on the heater control panel improves the visibility.
RELIABLE VISUAL FIELD (IMPROVEMENT IN SAFETY) Achievement of ventilation system to defog windows by increasing the fresh air intake duct area on the front deck and adopting a large air vent Windshield defogging speed improvement derived from increase in air volume and wind speed by adopting a blower type defroster and high performance heater
IMPROVEMENTS IN FUEL ECONOMY Optimisation of engine idle speed according to air conditioner load Cooling fan speed varies on the air conditioner load, thus reducing the alternator load Installation of sub-cooling type condenser to improve heat exchanging efficiency
GLOBAL ENVIRONMENT PROTECTION Adoption of a new refrigerant system
IMPROVEMENTS IN SERVICE QUALITY Reduction of refrigerant gas leakage and improvement in serviceability by incorporating condenser and receiver
SPECIFICATION
Item | Specification
--- | ---
Heater unit type | Two-layer full blow air mix method
Heater control type | Rotary type
Air conditioner switch type | Push button type
Compressor type | Standard type | MSC90CA
Large capacity type | MSC105CA
Cooling output | 5.5 kw
Heating output | L.H. drive vehicles | 5.0 kw
R.H. drive vehicles | 5.5 kw
Refrigerant | Type | R134a (HFC-134a)
Charge quantity g | 530 - 570
CONSTRUCTION DIAGRAM

[55] HEATER, AIR CONDITIONER AND VENTILATION - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation