[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF FIT ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| SUNROOF FIT ADJUSTMENT Fully close the roof lid glass. Fully open the sunshade. Remove the decoration cover. (Refer to .)
| To adjust the roof lid glass in the front/back or left/right direction, loosen the nuts securing the roof lid glass assembly, then move the roof lid glass assembly to the front/back or left/right. Check to see that the space between the roof lid glass and body is even across the entire circumference. Adjust the roof lid glass height according to the number of the adjusting plate pieces. Check to see that the height of the roof lid glass is even with the body. After adjustment, check to be sure that the sunroof operates smoothly.

[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF FIT ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation