[55A] HEATER, AIR CONDITIONER AND VENTILATION - - EVAPORATOR ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

EVAPORATOR ASSEMBLY

REMOVAL AND INSTALLATION
Pre-removal and Post-installation Operation Refrigerant draining and Refilling (Refer to Charging and Discharging ). Air cleaner cover and air flow sensor assembly Removal and Installation (Refer to GROUP 15, Air cleaner <2400-except MIVEC>, <2400-MIVEC>).
|  |  | Removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Flexible suction hose connection
<<A>> |  | 2. | Liquid pipe B connection
<<A>> |  | 3. | Expansion valve cover
<<A>> |  | 4. | Expansion valve
<<A>> |  | 5. | Joint
|  | 6. | O ring
|  | • | Glove box (Refer to GROUP 52A, Instrument Panel <L.H. drive vehicles>, <R.H. drive vehicles>).
|  | 7. | Joint duct
|  | • | Foot duct <driver's side>
|  | 9. | Front floor console lower side cover
|  | 10. | Evaporator cover
|  | 11. | Air thermo sensor clip
|  | 12. | Air thermo sensor
|  | 13. | Evaporator
| REMOVAL SERVICE POINT
| <<A>> FLEXIBLE SUCTION HOSE AND LIQUID PIPE B DISCONNECTION CAUTION As the compressor oil and receiver are highly moisture absorbent, use a non-porous material to plug the hose and nipples. To prevent the entry of dust or other foreign bodies, plug the dismantled hose and the nipples of the expansion valves.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - EVAPORATOR ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation