[14] ENGINE COOLING - - ON-VEHICLE SERVICE - RADIATOR CAP VALVE OPENING PRESSURE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| RADIATOR CAP VALVE OPENING PRESSURE CHECK NOTE: Be sure that the cap is clean before testing. Rust or other foreign material on the cap seal will cause an improper reading.
| Use a cap adapter to attach the cap to the tester. Increase the pressure until the indicator of the gauge stops moving. Minimum limit: 83 kPa Standard value: 93 - 123 kPa Replace the radiator cap if the reading does not remain at or above the limit.

[14] ENGINE COOLING - - ON-VEHICLE SERVICE - RADIATOR CAP VALVE OPENING PRESSURE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation