[14] ENGINE COOLING - - ON-VEHICLE SERVICE - COOLING FAN MOTOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| COOLING FAN MOTOR CHECK
| Remove the cooling fan motor connector. Check to see that the fan motor of the radiator turns when applying battery power between the connector terminals of the radiator fan motor. Also check to see that there is no abnormal sound coming from the cooling fan motor at this time. If the cooling fan motor is defective, replace it.

[14] ENGINE COOLING - - ON-VEHICLE SERVICE - COOLING FAN MOTOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation