[11E] ENGINE MECHANICAL <4G69> - - ON-VEHICLE SERVICE - MANIFOLD VACUUM CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| MANIFOLD VACUUM CHECK
| Before inspection, set the vehicle to the pre-inspection condition. Turn the ignition switch to the "LOCK" (OFF) position and then connect the MUT-II/IIII to the diagnosis connector or connect a tachometer to the engine speed detection connector.
| Disconnect the ventilation hose from the PCV valve, and connect a vacuum gauge to the ventilation hose. Plug the PCV valve. Start the engine and check that idle speed is within the standard valve. Standard value : 680 ± 100 r/min Check the intake manifold vacuum. Limit: Minimum 60 kPa Turn the ignition switch to the "LOCK" (OFF) position. Remove the vacuum gauge and then connect the ventilation hose. Remove the MUT-II/III.

[11E] ENGINE MECHANICAL <4G69> - - ON-VEHICLE SERVICE - MANIFOLD VACUUM CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation