[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 26: CD cannot be Inserted. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 26: CD cannot be Inserted.
DIAGNOSIS PROCEDURE
STEP1. Check that a CD has been already loaded. Q: Has a CD been already loaded? NO: Go to Step 2. YES: Take out the CD (If the CD can not be ejected, refer to INSPECTION PROCEDURE 30 ). Check that a CD can be inserted.
STEP 2. Check how a CD is inserted. Ensure that the ignition switch is at "ACC" or "ON". NOTE: If you try to load a CD when the ignition switch is at the positions other than "ACC" or "ON", the CD will not be inserted completely and then rejected. Q: If you try to load the CD, does the CD stops halfway and then rejected? YES: Refer to INSPECTION PROCEDURE 30 . NO: Go to Step 3.
STEP3. Check after the CD is loaded. NOTE: Even though the CD is loaded, "E" (error) is sometimes displayed with the CD rejected because of vibration/shock or dew on the CD face or optical lens. Q: Though the CD is inserted completely, is "E" (error) displayed and the CD ejected? YES: Go to Step 4. NO: The procedure is complete.
STEP 4. Check the CD. Check the CD for the conditions below: Is the CD loaded with its label facing down? Is the recorded face dirty or scratched? Is there dew on the recorded face? Q: Is the CD in good condition? YES: Go to Step 5. NO: The original CD is defective. Check that a CD can be inserted.
STEP 5. Check again using a normal CD, which is not dirty or scratched. Load another normal CD. Check that the CD player recognizes and play the CD. Q: When you substitute another normal CD, is the CD loaded correctly? YES: The original CD is defective. Check that a CD can be inserted. NO: Replace the radio with CD player. The procedure is complete.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 26: CD cannot be Inserted. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation