[34] REAR SUSPENSION - - ON-VEHICLE SERVICE - LOWER ARM PILLOW BALL BUSHING AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| LOWER ARM PILLOW BALL BUSHING AXIAL PLAY CHECK Raise the vehicle. Remove the stabilizer link and shock absorber from the lower arm assembly. Move the lower arm up and down with your hands to check for an excessive play in the axial direction of the pillow ball bushing. If there is an excessive play, replace the lower arm pillow ball bushing (Refer to ). After inspection, install the stabilizer link and shock absorber to the lower arm assembly (Refer to ).

[34] REAR SUSPENSION - - ON-VEHICLE SERVICE - LOWER ARM PILLOW BALL BUSHING AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation