[33] FRONT SUSPENSION - - STABILIZER BAR - STABILIZER LINK BALL JOINT DUST COVER REPLACEMENT <2000-DOHC AND 2400> | PRINT PAGE / INDEX / PRIOR / NEXT

| STABILIZER LINK BALL JOINT DUST COVER REPLACEMENT <2000-DOHC AND 2400> Only when the dust cover is damaged accidentally during service work, replace the dust cover as follows:
| Remove the clip ring and the dust cover. Apply specified grease to the inside of a new dust cover. Specified grease: Multipurpose grease SAE J310, NLGI No.2 or equivalent Wrap plastic tape around the stabilizer link stud, and then install the dust cover to the stabilizer link. Secure the dust cover by the clip ring. Check the dust cover for cracks or damage by pushing it with finger.

[33] FRONT SUSPENSION - - STABILIZER BAR - STABILIZER LINK BALL JOINT DUST COVER REPLACEMENT <2000-DOHC AND 2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation