[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A1. CHECK V-BELT FOR CRACKS, FRAYING, WEAR, AND ADJUST ITS TENSION | PRINT PAGE / INDEX / PRIOR / NEXT

OPERATIONS INSIDE THE ENGINE COMPARTMENT

| A1. CHECK V-BELT FOR CRACKS, FRAYING, WEAR, AND ADJUST ITS TENSION
| V-BELT CONDITION Check the whole rounds of the V-belt for cracks, fraying and wear.
| V-BELT TENSION
| Make sure that the indicator mark is with in the area marked with A in the illustration. CAUTION Check the drive belt tension after turning the crankshaft clockwise one turn or more. If the mark is out of the area, replace the drive belt. NOTE: The drive belt tension check is not necessary as auto-tensioner is adopted

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A1. CHECK V-BELT FOR CRACKS, FRAYING, WEAR, AND ADJUST ITS TENSION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation