[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G69>
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>A<< | 1. | Oxygen sensor <Vehicles for Hong Kong, Brunei, Singapore and Malaysia>
|  | 2. | Exhaust manifold cover
|  | • | Front exhaust pipe (Refer to ).
|  | 3. | Exhaust manifold bracket B <Vehicles for Hong Kong, Brunei, Singapore and Malaysia>
|  | 4. | Exhaust manifold
|  | 5. | Exhaust manifold gasket
|  | 6. | Exhaust manifold bracket A <Vehicles for Hong Kong, Brunei, Singapore and Malaysia>
| REMOVAL SERVICE POINT
| <<A>> OXYGEN SENSOR REMOVAL
| Use special tool oxygen sensor wrench (MD998770) to remove the oxygen sensor.
| INSTALLATION SERVICE POINT
| >>A<< OXYGEN SENSOR INSTALLATION
| Use special tool oxygen sensor wrench (MD998770) to install the oxygen sensor.

[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation