[35A] BASIC BRAKE SYSTEM - - REAR DISC BRAKE ASSEMBLY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Lock pin
|  | 2. | Bushing
|  | 3. | Guide pin
|  | 4. | Caliper support
|  | 5. | Pin boot
|  | 6. | Boot ring
<<A>> |  | 7. | Piston
<<A>> |  | 8. | Piston boot
<<B>> |  | 9. | Piston seal
|  | 10. | Caliper body
|  | 11. | Pad and wear indicator assembly
|  | 12. | Inner shim
|  | 13. | Clip
|  | 14. | Pad assembly
|  | 15. | Outer shim
LUBRICATION POINTS
| DISASSEMBLY SERVICE POINTS When disassembling the disc brakes, disassemble both sides (left and right) as a set.
| <<A>> PISTON BOOT/PISTON REMOVAL
| CAUTION Blow air little by little to remove the piston. The piston will rush out if a force of air is applied suddenly. Place a piece of wood, etc. against the caliper body as shown. Blow compressed air through the brake hose to remove the piston boot and piston.
| <<B>> PISTON SEAL REMOVAL CAUTION Do not use a flat-tipped screwdriver or similar tool to remove piston seal. These may damage the inner side of the cylinder.
| Remove the piston seal with your finger tip. Clean the piston surface and inner cylinder with alcohol or brake fluid DOT 3 or DOT 4.

[35A] BASIC BRAKE SYSTEM - - REAR DISC BRAKE ASSEMBLY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation