[15] INTAKE AND EXHAUST - - AIR INTAKE SYSTEM - INTERCOOLER <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

INTERCOOLER <4G63-DOHC>
The air-cooled intercooler is installed on the upper part of the engine to lower the intake air temperature after supercharging, allowing to increase the engine power. In addition, it has the following features. The optimized fin shape and installation of the heat protection panel increase the cooling capacity. Environmentally friendly unleaded rubber materials are used to make the intercooler air hose.
CONSTRUCTION DIAGRAM

[15] INTAKE AND EXHAUST - - AIR INTAKE SYSTEM - INTERCOOLER <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation