[23] AUTOMATIC TRANSMISSION - - ELECTRONIC CONTROL SYSTEM - EEPROM <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

ELECTRONIC CONTROL SYSTEM

EEPROM <4G69> Because EEPROM has been used, even if the battery terminals or control unit connectors are disconnected, the necessary learned values are stored in the engine-A/T-ECU to prevent a loss of shift quality. (Initialisation is available by MUT-II/III).

[23] AUTOMATIC TRANSMISSION - - ELECTRONIC CONTROL SYSTEM - EEPROM <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation