[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

| DIAGNOSIS FUNCTION
| N RANGE LAMP SYSTEM
| If there is a problem with any of the A/T system, the N range lamp will flash at a rate of approximately once per second. If the N range lamp is flashing at a rate of approximately once per second, check the diagnosis output. N range lamp flashing item Input shaft speed sensor system Output shaft speed sensor system Solenoid valve system Non-synchronization at various shift ranges A/T control relay system NOTE: If the "N" range lamp is flushing at a rate of approximately twice per second <Vehicles for Hong Kong spec.> or A/T fluid warning lamp is illuminating <Except for Hong Kong spec.>, the A/T fluid temperature is high. (It flushes when the fluid is approximately 125°C or more and goes off when the fluid is approximately 115°C or less.)
| METHOD OF READING THE DIAGNOSIS CODE Use the MUT-II/III to read the diagnosis code. (Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points .)
| METHOD OF ERASING THE DIAGNOSIS CODE Use the MUT-II/III to erase the diagnosis code. (Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points .)

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation