[11B] ENGINE OVERHAUL <4G6-SOHC> - - OIL PAN AND OIL PUMP - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| COUNTERBALANCE SHAFTS Check that the oil holes are not blocked.
| Check the journals for seizure, damage and defective contact with bearing. If any of these faults is found, replace the Counterbalance shaft, bearing and/or front case assembly.
| OIL PUMP Install the drive and driven gears in the front case.
| Measure the gear side clearance using a straight edge and thickness gauge. Standard values: Drive gear 0.08 - 0.14 mm Driven gear 0.06 - 0.12 mm

[11B] ENGINE OVERHAUL <4G6-SOHC> - - OIL PAN AND OIL PUMP - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation