[35A] BASIC BRAKE SYSTEM - - ON-VEHICLE SERVICE - BRAKE LINING AND BRAKE DRUM CONTACT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| BRAKE LINING AND BRAKE DRUM CONTACT CHECK Remove the brake drum. Remove the shoe and lining assembly (Refer to ).
| Chalk the inner surface of the brake drum and rub with the shoe and lining assembly. Replace the shoe and lining assembly or brake drums if there are any irregular contact areas. NOTE: Clean off chalk after check.

[35A] BASIC BRAKE SYSTEM - - ON-VEHICLE SERVICE - BRAKE LINING AND BRAKE DRUM CONTACT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation