[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D5. CHECK BRAKE SHOE LININGS AND DRUMS FOR WEAR | PRINT PAGE / INDEX / PRIOR / NEXT

| D5. CHECK BRAKE SHOE LININGS AND DRUMS FOR WEAR
| BRAKE LINING THICKNESS CHECK Remove the brake drum.
| Measure the thickness of the brake lining at the place worn the most. <Vehicles with drum brake> Standard value (A): 4.9 mm Limit (A): 1.0 mm <Vehicles with drum-in-disc brake> Standard value (A): 2.8 mm Limit (A): 1.0 mm Replace the shoe and lining assembly as an axle set if brake lining thickness is less than the limit.
| BRAKE DRUM INSIDE DIAMETER CHECK Remove the brake drum.
| Measure the inside diameter of the brake drum at two or more locations. <Vehicles with drum brake> Standard value (A) : 228.6 mm Limit (A) : 230.6 mm <Vehicles with drum-in-disc brake> Standard value (A): 168.0 mm Limit (A): 169.0 mm Replace the brake drum when the inside diameter exceeds the limit value or the brake drum is worn unevenly.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D5. CHECK BRAKE SHOE LININGS AND DRUMS FOR WEAR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation