[14] ENGINE COOLING - - THERMOSTAT - REMOVAL AND INSTALLATION <4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G6-DOHC>
Pre-removal and Post-installation Operation Engine Coolant Draining and Refilling (Refer to ). Air Cleaner Removal and Installation (Refer to GROUP 15, Air Cleaner ). Battery Removal and Installation
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Fuel pressure control solenoid valve connector
|  | 2. | Waste gate solenoid valve connector
|  | 3. | Engine coolant temperature gauge unit connector
|  | 4. | Engine coolant temperature sensor connector
|  | 5. | Control wiring harness connection
|  | 6. | Harness bracket
<<A>> | >>B<< | 7. | Radiator lower hose connection
|  | 8. | Water inlet fitting
| >>A<< | 9. | Thermostat
| REMOVAL SERVICE POINT
| <<A>> RADIATOR LOWER HOSE DISCONNECTION
| Make mating marks on the radiator hose and the hose clamp. Disconnect the radiator hose.
| INSTALLATION SERVICE POINTS
| >>A<< THERMOSTAT INSTALLATION CAUTION Make absolutely sure that no oil adheres to the rubber ring of the thermostat. Also do not fold or scratch the rubber ring during installation.
| Install the thermostat so that the jiggle valve is facing straight up. Be careful not to fold or scratch the rubber ring.
| >>B<< RADIATOR LOWER HOSE CONNECTION
| Insert each hose as far as the projection of the water inlet fitting. Align the mating marks on the radiator hose and hose clamp, and then connect the radiator hose.

[14] ENGINE COOLING - - THERMOSTAT - REMOVAL AND INSTALLATION <4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation