[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - PULSE CHECK PROCEDURE | PRINT PAGE / INDEX / PRIOR / NEXT

| PULSE CHECK PROCEDURE The input signals (signals other than communication line signals), which are compatible with the SWS monitor by using the MUT-II/III or voltmeter, can be confirmed by the Pulse Check (Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points). Use the MUT-II/III or voltmeter to check the following input signals. NOTE: If a problem is found in the "Pulse check", refer to the Problems during Input Signal Check <Service data, function diagnosis or pulse check> (Refer to ).
| Switches and their conditions, which are applicable for Pulse Check
Input signals | Requirements for sounding buzzer
--- | ---
INTERIOR LAMP LOADED SIGNAL | When a load is applied through multi-purpose fuse No.18

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - PULSE CHECK PROCEDURE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation