[8] REFERENCE MATERIAL - - SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - AIR BAG | PRINT PAGE / INDEX / PRIOR / NEXT

SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - AIR BAG
WARNING Improper service or maintenance of any component of the SRS and any SRS-related component, can lead to personal injury or death to service personnel (from inadvertent firing of the air bag or to the driver and passenger (from rendering the SRS inoperative). The SRS components and seat belt with pre-tensioner should not be subjected to heat, so remove the SRS-ECU, driver’s and front passenger’s air bag modules, clock spring, side air bag modules, and seat belt pre-tensioner before drying or baking the vehicle after painting. SRS-ECU, air bag module, clock spring: 93°C or more Seat belt pre-tensioner :90°C or more Service or maintenance of any SRS component and SRS-related component must be performed only at an authorized MITSUBISHI dealer. MITSUBISHI dealer personnel must thoroughly review the chassis workshop manual, and especially its GROUP 52B - Supplemental Restraint System (SRS), before beginning any service or maintenance of any component of the SRS and any SRS-related component.

[8] REFERENCE MATERIAL - - SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - AIR BAG | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation