[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SYSTEM OPERATION - FRONT IMPACT SENSOR | PRINT PAGE / INDEX / PRIOR / NEXT

| FRONT IMPACT SENSOR
| The front impact sensor for 2400 engine is installed on the outside of the headlamp support in the engine room. And that for 2000 engine is installed on the side member. In a collision, the contact in the front impact sensor turns ON and an output signal is send to the SRS-ECU. A resistor is connected to the front impact sensor in parallel with the contact for fault diagnosis.

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SYSTEM OPERATION - FRONT IMPACT SENSOR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation