[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - FUEL PUMP CONNECTOR DISCONNECTION (HOW TO REDUCE PRESSURIZED FUEL LINES) | PRINT PAGE / INDEX / PRIOR / NEXT

| FUEL PUMP CONNECTOR DISCONNECTION (HOW TO REDUCE PRESSURIZED FUEL LINES) The service procedure is the same as the vehicles with 4G63- engine. (Refer to GROUP 13A - On-vehicle Service ).

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - FUEL PUMP CONNECTOR DISCONNECTION (HOW TO REDUCE PRESSURIZED FUEL LINES) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation