[11D] ENGINE OVERHAUL <4G6-DOHC> - - INLET MANIFOLD - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

INLET MANIFOLD

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
| >>B<< | 1. | Manifold differential pressure (MDP) sensor
| >>A<< | 2. | Inlet manifold stay
|  | 3. | Alternator brace stay
|  | 4. | Inlet manifold
|  | 5. | Inlet manifold gasket
|  | 6. | Detonatoin sensor
| INSTALLATION SERVICE POINTS
| >>A<< INLET MANIFOLD STAY INSTALLATION
| Tighten the bolts to the specified torque 31 ± 3 N·m on both ends after making sure that the stay is in close contact with the bosses on the inlet manifold and cylinder block.
| >>B<< MDP SENSOR INSTALLATION CAUTION Install the MDP sensor carefully not to give it a shock. Do not use the sensor that has fallen to floor or any other surface.

[11D] ENGINE OVERHAUL <4G6-DOHC> - - INLET MANIFOLD - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation