[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM>

GENERAL INFORMATION By using the auto-cruise control, the driver can drive at preferred speeds in a range of approximately 40 to 200 km/h without depressing the accelerator pedal. For this auto-cruise control system, in conjunction with the electronic throttle valve control system, the engine-A/T-ECU electronically controls the throttle valve. CONSTRUCTION DIAGRAM

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation