[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 24: Malfunction of the Auto Reverse. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 24: Malfunction of the Auto Reverse.
DIAGNOSIS PROCEDURE
STEP 1. Check that the tape player works normally when the tape is changed. NOTE: Ensure that the tape label is not loose, that the tape itself is not deformed and that the tape is tightly wound. Also, tape of C-120 or greater length often get caught in the mechanism and should not be used. Q: Does the tape player work normally if the tape is changed? YES: The tape used is defective. The auto reverse function should operate normally. NO: Go to Step 2.
STEP 2. Check that the problem only occur while the vehicle is being driven. Q: Does the problem only occur while the vehicle is being driven? YES: Go to Step 3. NO: Replace the radio and tape player. The auto reverse function should operate normally.
STEP 3. Check that the tape player is properly installed to the vehicle. Q: Is the tape player properly installed to the vehicle? YES: Replace the radio and tape player. The auto reverse function should operate normally. NO: Repair the installation condition. The procedure is complete.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 24: Malfunction of the Auto Reverse. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation