[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - CHECK TROUBLE BY USING THE INPUT SIGNAL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

CHECK TROUBLE BY USING THE INPUT SIGNAL CHECK
<Pulse check>
If a problem is found in the Service Data or Pulse Check inspection, observe the table below.
Symptom | Inspection procedure number | Reference page
--- | --- | ---
The ignition switch (ACC) signal is not received. | P-1 |
The ignition switch (IG1) signal is not received. | P-2 |
The inhibitor switch (reverse position) signal is not received. | P-3 |
The driver's door switch signal is not received. | LH drive vehicles | P-4 |
RH drive vehicles |
Column switch (lighting and turn-signal lamp switch) | The tail lamp switch signal is not received. | P-5 |
The headlamp switch signal is not received.
The dimmer switch signal is not received.
The passing switch signal is not received.
The turn-signal lamp switch (LH) signal is not received.
The turn-signal lamp switch (RH) signal is not received.
Column switch (windshield wiper/washer and rear wiper/washer switch) | The windshield mist wiper switch signal is not received. | P-6 |
The windshield intermittent wiper switch signal is not received.
The windshield low-speed wiper switch signal is not received.
The windshield high-speed wiper switch signal is not received.
The windshield washer switch signal is not received.
The rear wiper switch signal is not received.
The rear washer switch signal is not received.
The windshield intermittent wiper volume signal is not received. | P-7 |
Power window main switch <vehicles for Argentina> | When the power window main switch is operated, the switch signals are not received. | P-8 |
Sunroof | When the sunroof switch is operated, the switch signals are not received. | P-9 |
The front fog lamp switch signal is not received. | P-10 |
The rear fog lamp switch signal is not received. | P-11 |
The key reminder switch signal is not received. | P-12 |
The hazard warning lamp switch signal is not received. | P-13 |
All the door switch signals are not received. | LH drive vehicles | P-14 |
RH drive vehicles |
The driver's door lock actuator switch signal is not received. | LH drive vehicles | P-15 |
RH drive vehicles |
The vehicle speed signal is not received. <Except vehicles for GCC> | P-16 |
Each switch signal of the keyless entry transmitter is not received. | P-17 |
The interior lamp loaded signal is not detected. | P-18 |
The passenger’s door lock key cylinder switch signal is not detected. | LH drive vehicles | P-19 |
RH drive vehicles |
The passenger’s door switch signal is not detected. <vehicles for Australia> | P-20 |

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - CHECK TROUBLE BY USING THE INPUT SIGNAL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation