[33] FRONT SUSPENSION - - STRUT ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

STRUT ASSEMBLY

REMOVAL AND INSTALLATION
CAUTION For vehicles with ABS, be careful when handling the pole piece at the tip of the front ABS sensor so as not to damage it by striking against other parts.
Pre-removal Operation Washer Tank Assembly Removal (2000: Refer to GROUP 51, Windshield Wiper and Washer /2400: Refer to GROUP 51, Windshield Wiper and Washer ). <Pre-removal of the strut assembly (RH)> | Post-installation Operation Washer Tank Assembly Installation (2000: Refer to GROUP 51, Windshield Wiper and Washer /2400: Refer to GROUP 51, Windshield Wiper and Washer ). <Post-installation of the strut assembly (RH)> Front Wheel Alignment Adjustment (Refer to ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Front ABS sensor harness bracket <Vehicles with ABS>
|  | 2. | Brake hose bracket
|  | 3. | Knuckle connection
|  | 4. | Strut mounting nut
|  | 5. | Insulator clip <2000-DOHC and 2400>
|  | 6. | Stiffener plate <2000-DOHC and 2400>
|  | 7. | Strut assembly

[33] FRONT SUSPENSION - - STRUT ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation