[54A] CHASSIS ELECTRICAL - - THEFT ALARM <Vehicles for Hong Kong spec.> - THEFT ALARM SYSTEM TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

THEFT ALARM <Vehicles for Hong Kong spec.>

THEFT ALARM SYSTEM TROUBLESHOOTING
The theft alarm system is controlled by the Smart Wiring System (SWS). For troubleshooting, refer to respective Groups below. Not using SWS monitor: GROUP 54B, Troubleshooting .

[54A] CHASSIS ELECTRICAL - - THEFT ALARM <Vehicles for Hong Kong spec.> - THEFT ALARM SYSTEM TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation