[34] REAR SUSPENSION - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Toe-in | At the centre of tyre tread mm | 3 ± 2
Toe-angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30' (Difference between right and left within 30')
Thrust angle | 0°00' ± 09'
Control link pillow ball bushing starting torque N·m | 0.5 - 3.0
Upper arm pillow ball bushing starting torque N·m | 0.5 - 3.0
Lower arm pillow ball bushing starting torque N·m | 0.5 - 3.0
Protruding length of stabilizer link thread part mm | 2000-SOHC | 6 - 8
Stabilizer link ball joint turning torque N·m | 2000-SOHC | 0.5 - 1.5
2000-DOHC and 2400 | 1.7 - 3.1

[34] REAR SUSPENSION - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation