[27] REAR AXLE - - DIFFERENTIAL | PRINT PAGE / INDEX / PRIOR / NEXT

DIFFERENTIAL
The differential specifications are established as follows.
SPECIFICATIONS
Item | Specification
--- | ---
Reduction gear type | Hypoid gear
Reduction ratio | 3.312
Differential gear type (Type × number of gears) | Side gear | Straight bevel gear × 2
Pinion gear | Straight bevel gear × 2
Number of teeth | Drive gear | 53
Drive pinion | 16
Side gear | 14
Pinion gear | 10
Bearing (Outside diameter × inside diameter) mm | Side | 72 × 35
Front | 62 × 25
Rear | 72 × 35
Differential gear oil | Type | Hypoid gear oil API classification GL-5 or higher SAE viscosity No.90, 80W
Amount L | 0.55
DIFFERENTIAL MOUNT
<2000-Turbo> The differential carrier is supported by the differential mount bracket and differential support member on the front side, and is secured to the rear suspension crossmember with a bushing. It is supported by the differential support arm at the rear, and is secured to the rear suspension crossmember with a bushing. The differential support arm bushings and differential support member bushings to absorb vibration from the suspension.
<2400> The differential carrier is supported by the differential mount bracket on the front side, and is secured to the rear suspension crossmember with a bushing. It is supported by the differential support arm at the rear, and is secured to the rear suspension crossmember with a bushing. The differential support arm bushings to absorb vibration from the suspension. The weight is used to reduce differential gear noise.

[27] REAR AXLE - - DIFFERENTIAL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation