[42] BODY - - DOOR - WINDOW GLASS REGULATOR | PRINT PAGE / INDEX / PRIOR / NEXT

WINDOW GLASS REGULATOR
The power window has the following features. The window glass regulator is a compact and light-weight wire winding type. The new power window system is adopted. The system enables to open the power window even if the vehicle is submerged <Vehicles for Hong Kong spec and Argentina>. The anti-pinch function is adopted <Vehicles for Hong Kong spec and Argentina>. The power window timer function is adopted <Except vehicles for Argentina>. The power window lock switch is adopted.
CONSTRUCTION DIAGRAM
DESCRIPTION OF STRUCTURE AND OPERATION
POWER WINDOW SYSTEM <VEHICLES FOR HONG KONG SPEC AND ARGENTINA> If the vehicle should be submerged in river or sea, each power window can be opened for a while to improve safety. "For a while" means that the period while the operation voltage is supplied from the battery to the power windows. The duration varies depending on the severity of the submergence, battery capacity, and battery charging level. The power window switch has a waterproofing structure which prevents water such as rain drops from entering via the upper side. If water should be entered, it is drained through the hole located on the lower area of the switch. No water may be accumulated. NOTE: Only if the whole switch is submerged in water, the switch determines that the vehicle is submerged.
ANTI-PINCH FUNCTION <VEHICLES FOR HONG KONG SPEC AND ARGENTINA> The power window with the safety mechanism is adopted. If any obstacle such as a hand or a head is detected to be pinched during a window glass closing operation, the window glass is opened by approximately 150 mm to improve safety.
POWER WINDOW SWITCH The power window switch employs the push-pull operation method to improve safety. To close a door window glass, press in the switch knob, and to open, pull it up. The one-touch mechanism is adopted to the driver power window switch to fully open the driver's door window glass in a single operation <Except vehicles for Hong Kong spec and Argentina>. The one-touch mechanism is adopted to the driver's power window switch to fully open or close any door window glass in a single operation <Vehicles for Hong Kong and Argentina>.
POWER WINDOW TIMER FUNCTION The power window has a timer function which allows the window glass to be closed or opened after the ignition switch is turned OFF (Refer to GROUP 54B, SMART WIRING SYSTEM ). During the timer operation, if the driver's door is opened, the time is extended by 30 seconds from the moment. However, the timer is expired when the driver's door is closed during the extended time <Except vehicles for Australia, New Zealand (2400) and Argentina>. During the timer operation, if the driver's door or front passenger's door is opened, the timer is expired at the moment <Vehicles for Australia and New zealand (2400)>. During the timer operation, if the driver's door is opened, the time is extended by 30 seconds from the moment. However, the timer is expired when the driver's door is closed during the extended time. The timer setting can be changed to zero, 30 seconds, 3 minutes, or 10 minutes by the adjustment function. The initial setting at factory is 30 seconds <Vehicles for Hong Kong spec>. NOTE: *: The power window timer setting can be changed as an adjustment function (Refer to GROUP 54B, SMART WIRING SYSTEM ).
POWER WINDOW LOCK SWITCH The driver power window switch is equipped with the lock switch. This switch inhibits the opening/closing operation of the door window glass by the front passenger's power window switch or rear power window switches. The ON function of the lock switch can be changed to "Operation of all seats is prohibited," or "Operation of any seats other than the driver's seat is inhibited" by the adjustment function. The initial setting at factory is "When locked, operation from all seats is possible" <Vehicles for Hong Kong spec>. NOTE: *: The power window lock switch operation can be changed as an adjustment function (Refer to GROUP 54B, SMART WIRING SYSTEM ).

[42] BODY - - DOOR - WINDOW GLASS REGULATOR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation