[11C] ENGINE MECHANICAL <4G6-DOHC> - - ON-VEHICLE SERVICE - IDLE SPEED CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| IDLE SPEED CHECK
| Before inspection, set the vehicle to the pre-inspection condition. Turn the ignition switch to "LOCK" (OFF) position. Connect the MUT-II/III to the diagnosis connector or connect a tachometer to the engine speed detection connector. Connect a timing light.
| Start the engine and let it run at idle. Check that ignition timing is at the standard value. Standard value: approximately 5° BTDC Check the idle speed. Standard value: 750 ± 100 r/min NOTE: The idle speed is controlled automatically by the idle speed control system. When using the MUT-II/III, select item No. 22 and take a reading of the idle speed. If the idle speed is outside the standard value, inspect the MPI system (Refer to GROUP 13A - Troubleshooting - Inspection chart for diagnosis code ).

[11C] ENGINE MECHANICAL <4G6-DOHC> - - ON-VEHICLE SERVICE - IDLE SPEED CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation