[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A13. REPLACE AIR CLEANER ELEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| A13. REPLACE AIR CLEANER ELEMENT The air cleaner element will become dirty and loaded with dust during use, and the filtering effect will be substantially reduced. Replace it with a new one.
| Unclasp the air cleaner cover clip. Remove the air cleaner element and install a new one. Be sure to close the air cleaner cover completely when clamping it.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A13. REPLACE AIR CLEANER ELEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation