[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - FUEL GAUGE UNIT CHECK <4WD> | PRINT PAGE / INDEX / PRIOR / NEXT

| FUEL GAUGE UNIT CHECK <4WD> Remove the fuel pump and gauge unit and the remove the fuel gauge unit. (Refer to GROUP 13D, Fuel Tank <except for Brazil and Chile> or <vehicles for brazil and Chile>).
| FUEL GAUGE UNIT RESISTANCE
| Check that resistance value between the fuel gauge terminal and earth terminal is at the standard value when the fuel pump and gauge unit or fuel gauge unit float is between position F (highest) and position E (lowest). Standard value: Float position F: 1.5 ± 0.5 Ω Float position E: 55 ± 1.5 Ω Check that resistance value changes smoothly when the float moves slowly between position F (highest) and position E (lowest). If all checks are correct, go to fuel pump and gauge unit or fuel gauge unit float height check. If any check is not correct, replace the fuel pump and gauge unit or fuel gauge unit.
| FUEL GAUGE UNIT FLOAT HEIGHT
| Move the float and measure height A at position "F" (highest) and B at position "E" (lowest) with the float arm touching stopper. Standard value <Fuel pump and gauge unit>: Float position A: 36.7 ± 2 mm Float position B: 149.6 ± 2 mm Standard value <Fuel gauge unit>: Float position A: 23.4 ± 2 mm Float position B: 194.2 ± 2mm If all checks are correct, go to fuel pump and gauge unit or fuel gauge unit float height check. If any check is not correct, replace the fuel pump and gauge unit or fuel gauge unit.

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - FUEL GAUGE UNIT CHECK <4WD> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation