[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - FUEL GAUGE UNIT CHECK <2WD> | PRINT PAGE / INDEX / PRIOR / NEXT

| FUEL GAUGE UNIT CHECK <2WD> Remove the fuel pump module and the remove the fuel gauge unit. (Refer to GROUP 13D, Fuel Tank ).
| FUEL GAUGE UNIT RESISTANCE
| Check that resistance value between the fuel gauge terminal and earth terminal is at the standard value when the fuel gauge unit float is between position F (highest) and position E (lowest). Standard value: Float position F : 3 ± 0.6 Ω Float position E : 110 ± 2.5 Ω Check that resistance value changes smoothly when the float moves slowly between position F (highest) and position E (lowest). If all checks are correct, go to fuel gauge unit float height check. If any check is not correct, replace the fuel gauge unit.
| FUEL GAUGE UNIT FLOAT HEIGHT
| Move the float and measure height A at position F (highest) and B at position E (lowest) with the float arm touching stopper. Standard value: Position F (A) : 35.4 mm ± 2 mm Position E (B) : 186.7 mm ± 2 mm If all checks are correct, go to fuel gauge unit float height check. If any check is not correct, replace the fuel gauge unit.

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - FUEL GAUGE UNIT CHECK <2WD> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation