[51] EXTERIOR - - HEADLAMP WASHER <Except vehicles for Hong Kong> - HEADLAMP WASHER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| HEADLAMP WASHER MOTOR CHECK
| Remove the headlamp washer motor connector. Check to see that the water is vigorously sprayed when connecting the positive battery terminal to terminal number 1 and terminal number 2 to the negative battery terminal.

[51] EXTERIOR - - HEADLAMP WASHER <Except vehicles for Hong Kong> - HEADLAMP WASHER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation