[54A] CHASSIS ELECTRICAL - - FOG LAMP - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

FOG LAMP

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Fog lamp aiming (vertical direction) | Within 45 mm (0.86°) to 75 mm (1.44°) below the vertical centre line ahead of fog lamp.

[54A] CHASSIS ELECTRICAL - - FOG LAMP - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation