[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - OIL CONTROL VALVE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| OIL CONTROL VALVE CHECK
| OPERATION CHECK
| Disconnect the oil control valve connector. CAUTION To prevent the coil from burning, keep the duration of the voltage application as short as possible. Apply battery voltage to the terminals of the connector at the oil control valve, and make sure the oil control valve makes a clicking sound.
| MEASUREMENT OF RESISTANCE BETWEEN TERMINALS Disconnect the oil control valve connector. Measure the resistance between the terminals of the connector at the oil control valve. Standard value: 6.9 - 7.9 Ω (at 20°C) If resistance is outside the standard value, replace the oil control valve.

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - OIL CONTROL VALVE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation