[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-7: The windshield intermittent wiper volume signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE P-7: The windshield intermittent wiper volume signal is not received.
| CAUTION Whenever the ECU is replaced, ensure that the input signal circuit is normal.
| COMMENTS ON TROUBLE SYMPTOM The intermittent wiper interval is calculated in accordance with the input signal from the windshield intermittent wiper volume. If this signal is abnormal, the wiper interval can not be adjusted.
| POSSIBLE CAUSES Malfunction of the column switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Connector check: C-310 column switch connector Q: Is the check result normal? YES: Go to Step 2. NO: Repair the connector.
| Step 2. Measure the resistance at the C-310 column switch connector. Disconnect the connector, and measure at the column switch side. Resistance between C-310 column switch connector terminal No.6 and body earth OK: The resistance should rise from 0 to 1 kΩ when the windshield intermittent wiper volume is rotated from "Fast" to "Slow". Q: Is the check result normal? YES: Go to Step 3. NO: Replace the column switch.
| Step 3. Connector check: C-219 ETACS-ECU connector Q: Is the check result normal? YES: Go to Step 4. NO: Repair the connector.
| Step 4. Check the wiring harness between C-310 column switch connector terminal No.6 and C-219 ETACS-ECU connector terminal No.66. Check the input line for open circuit. Q: Is the check result normal? YES: Go to Step 5. NO: Repair the wiring harness.
| Step 5. Retest the system. Check that the windshield intermittent wiper volume is sending a correct signal. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-7: The windshield intermittent wiper volume signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation