[42] BODY - - KEYLESS ENTRY SYSTEM - TRANSMITTER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| TRANSMITTER BATTERY CHECK
| Measure the voltage of the battery. If the voltage of the battery is not within the standard value, replace the battery. Standard value:2.5 - 3.2 V

[42] BODY - - KEYLESS ENTRY SYSTEM - TRANSMITTER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation