[42] BODY - - TAILGATE - ON-VEHICLE SERVICE - TAILGATE HANDLE PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| TAILGATE HANDLE PLAY CHECK
| Check that the tailgate handle play satisfies the standard value. Standard value (A): 2.3 mm If it deviates from the standard value, remove the tailgate lower trim. Refer to GROUP 52A, Tailgate Trim . Remove the tailgate handle holder. Then adjust the play by changing the connecting point between the tailgate latch rod and the tailgate handle.

[42] BODY - - TAILGATE - ON-VEHICLE SERVICE - TAILGATE HANDLE PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation