[54A] CHASSIS ELECTRICAL - - HAZARD WARNING LAMP SWITCH - HAZARD WARNING LAMP SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| HAZARD WARNING LAMP SWITCH CONTINUITY CHECK
Switch position | Tester connection | Specified condition
--- | --- | ---
Released | 1 - 2 | Open circuit
Pressed | 1 - 2 | Less than 2 ohms

[54A] CHASSIS ELECTRICAL - - HAZARD WARNING LAMP SWITCH - HAZARD WARNING LAMP SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation