[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 16: Distortion on FM Only. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 16: Distortion on FM Only.
DIAGNOSIS PROCEDURE
STEP 1. Check with another broadcasting station. Q: Is there distortion when turning to another broadcasting station? YES: Go to Step 2. NO: The signal from that station is too weak.
STEP 2. Relocate the reception area and check. Q: When relocating the reception area does the distortion increase or decrease? YES: The cause may be multipath noise. NO: Repair or replace the radio and tape or CD player. Check that a distortion is resolved.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 16: Distortion on FM Only. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation