[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - SERVICE SPECIFICATION(S) | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATION(S)
Items | Standard value
--- | ---
Purge control solenoid valve coil resistance (at 20°C) Ω | 30 - 34 <4G63, 4G69 Except for Brazil and Chile>
22 - 26 <4G69 Vehicles for Brazil and Chile>
EGR control solenoid valve coil resistance (at 20°C) Ω | 29 - 35 <4G63, 4G69>
EGR valve coil resistance (at 20°C) Ω | 20 - 24 <4G69>

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - SERVICE SPECIFICATION(S) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation